Voltage Current

IP VP

t1 t 0

0